Nanjing\_CO2\_13C\_2013-2015.doc

(Update November 16, 2016)

0) Fair use policy: Kindly inform the appropriate Principal Investigators of how you are using site data and of any publication plans. If the Principal Investigators feel that they should be acknowledged or offered participation as authors, they will let you know and we assume that an agreement on such matters will be reached prior to publishing and/or use of the data for publication. If your work directly competes with the Principal Investigator's analysis they may ask that they have the opportunity to submit a manuscript before you submit the one that uses their data. In addition, when publishing, please acknowledge the agency that supported the research.

1) Contact info: xuhui.lee@yale.edu, phone 203-432-6271, fax 203-432-5023

wei.xiao@nuist.edu.cn, phone 86-15050575821

wangw@nuist.edu.cn, phone 86-15195915526

2) The mixing ratio of total atmospheric CO2 and 13C/12C ratio in reference to VPDB scale was measured continuously by a isotope analyzer based on wavelength-scanned cavity ring-down spectroscopy (model G1101-i, Picarro, Inc, Sunnyvale, California) in campus of Nanjing University of Information Science & Technology (32°12′ N, 118°43′ E), Nanjing, Jiangsu, China from February 2013 to August 2015. Details on the observation are given by Xu et al. 2016, available at http://yncenter.sites.yale.edu/publications

3) Each day have 48 records. Missing values are denoted by -9999.

4) Relevant references:

[1] Xu JP, X Lee, W Xiao, C Cao, SD Liu, XF Wen, JZ Xu, Z Zhang, JY Zhao (2016) Interpreting the 13C/12C ratio of carbon dioxide in an urban airshed in the Yangtze River Delta, China. In review.

5) Content and format of header records:

Sheet Nanjing\_CO2\_13C\_2013-2015

(:,1): Year

(:,2): Day, Day of year

(:,3): Hour, Local time ending, Beijing time

(:,4): Total CO2, molar ratio of total CO2 (12C and 13C) to dry air(calibrated, ppm; gaps filled with -9999)

(:,5): δ13C, 13C/12C ratio in delta notation in reference to VPDB scale (calibrated and corrected for water vapor interference, per mil, gaps filled with -9999)